Item 2: Develop standard PV generation profile
Joint IOUs’ Parameter Comparison
ICA Working Group
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Comparison for inputs used in parameters of NREL PVWATTS tool.
	System Info
	PG&E
	SDG&E
	SCE
	Notes

	DC System Size
	1 (normalized)
	 1(normalized)
	5.2
	Application Information (Average)

	Module Type
	Standard
	Standard
	standard
	Default

	Array Type
	Fixed
	Fixed
	fixed (roof mount)
	Application Information (Average)

	System Losses
	14%
	14%
	14%
	Default

	Tilt
	20 (res.)
15 (com/ind)
	18
	18 
	Application Information (Average)

	Azimuth 
	180
	180
	180
	Application Information (Average)

	DC to AC Ratio
	1.03
	1.15
	1.15
	Application Information (Average)

	PV Inverter Efficiency
	96%
	96%
	96.5%
	Application Information (Average)

	Ground Cover Ratio
	0.4
	0.4
	0.4
	Default



